# Changing control IP addresses

You can change the control IP address of an Security Engine without losing management connectivity.

When you change IP addressing, other connections between the different components might be temporarily lost. You must make sure that the connections return to normal after the IP address changes.
Note: We recommend that you do not use the IP address of an Aggregated Link interface as the primary or secondary control IP address of the Engine.