# Enable Web Access

You can enable and configure the feature in the properties of the Management Server or Web Access Server.

##

Note: To use Web Access for a Management Server or Web Access Server installed on a Linux platform, xvfb-run must be installed in /usr/bin.
Note: When Web Access is enabled, the Agentless ZTNA Application setup lets you to access SMC UI through FONE portal.
Note: Administrator must enable the ZTNA Connector to access the SMC, and add regular access policy rules to allow the traffic to the services behind the engine. For more information, see Engine Editor > Add-Ons > ZTNA Connector.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Select Network Elements.
2. Browse to Servers.
3. Right-click the Management Server or Web Access Server, then select Properties.
4. On the Web Access tab, select Enable.
5. Configure the settings, then click OK.