# Enable showing users on the Dashboard

To monitor users in the Dashboard view, you must enable the option in the global system properties.

##

The settings defined in the global system properties apply to all administrators in all Administrative Domains.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Select Settings > Global System Properties.
2. On the Global Options tab, select Show Users in the Dashboard View.
3. Configure the other settings in the User Information section.
4. Click OK.

## Global System Properties dialog box — Global Options tab

Use this tab to configure general settings for the SMC and Security Engines.

You can also use this tab to:

- Authorize McAfee® Global Threat Intelligence™ (McAfee GTI). Only administrators with unrestricted permissions (superusers) can enable McAfee GTI.
- Set the expiration time for one-time passwords that are generated when you save the initial configuration for an Security Engine.
- Import Snort configuration files globally to configure default settings for Snort inspection for all Security Engines.

All settings are optional.

Option | Definition
--- | ---
Enable McAfee Global Threat Intelligence (GTI) and McAfee Threat Intelligence Exchange (TIE) usage | When selected, enables McAfee GTI usage. Note: McAfee Threat Intelligence Exchange (TIE) is no longer supported in Security Engine 6.10 and higher.
One-Time Passwords Expire After | Defines the expiration time for one-time passwords that are generated when you save the initial configuration for an Security Engine. If the one-time password is not used, it automatically expires after the expiration time has elapsed. By default, one-time passwords expire after 30 days.
Snort Configuration | The externally created Snort configuration .zip file that contains the Snort configuration files and rules for Snort inspection. Click Browse to select a file. Click None to remove a previously imported file. Click Export to export the Snort configuration file. All Security Engines for which Snort inspection is enabled use the global Snort configuration by default. Settings in the Snort configuration .zip file for an individual Security Engine are combined with the settings in the global Snort configuration .zip file. If any configuration files in a Snort configuration .zip file for an individual Security Engine have the same files name and paths as configuration files in the global Snort configuration .zip file, the overlapping files in the global Snort configuration .zip file are ignored.
Distribution Points | Specify the URLs of the distribution points to prefetch CRLs and store them in the CRL Cache in advance. This allows for certificate validation to occur even if the network connection to the CRL Server is unavailable during the validation process. Note: The URLs specified here are shared with all Management Servers and Log Servers of the SMC.