# Enable outbound traffic management using element-based NAT

When you use element-based NAT for outbound traffic management, an Outbound Multi-Link element is automatically created based on the routing configuration.

## Before you begin

Configure routing with at least two NetLinks.

##

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Right-click an engine element and select Edit <element type>.
2. In the navigation pane on the left, browse to Policies > Element-based NAT.
3. From the Use Default NAT Address for Traffic from Internal Networks drop-down list, select Automatic.
4. Click Save and Refresh.