# Icons that indicate malfunctions

Engine hardware malfunction is indicated with an icon on top of the affected engine’s icon in the Status tree and on all top-level branches of the tree.

For more information about the hardware malfunction, select the engine in the Status tree, then click the Status tab in the Info pane.

Table 1. Hardware malfunction icons
Icon | Hardware status | Description
--- | --- | ---
| Warning | A predefined Warning level has been reached in hardware monitoring (for example, the remaining file system capacity is less than 15%). The system also generates a log entry.
| Alert | A predefined Alert level has been reached in hardware monitoring (for example, the remaining file system capacity is less than 5%). The system also generates an alert entry.

## Replication malfunction icon

In an environment with more than one Management Server, the configuration data is replicated to all Management Servers that are online. If the replication of configuration data among the Management Servers fails, an exclamation point on a yellow triangle is shown. You can see this icon on top of the Management Server’s icon in the Status tree for each Management Server that is not synchronized with the other Management Servers.