# Enable redirection of unauthenticated HTTP or HTTPS connections

To use browser-based user authentication, you must define some IPv4 or IPv6 Access rules.

##

Note: To redirect HTTPS traffic, you must enable TLS decryption for the traffic.

You must define the following IPv4 or IPv6 Access rules:

- An Access rule that allows all clients to access the logon page.
- An Access rule that allows authenticated users to establish HTTP or HTTPS connections.
- An Access rule that redirects unauthenticated HTTP or HTTPS traffic to the logon page.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Select Engine.
2. Browse to Policies > <Policy type>.
3. Right-click a policy, then select Edit <Policy name>.
4. Add the following Access rules:

   Table 1. Example Access rules for unauthenticated HTTP connections
   Source | Destination | Service | Action | Authentication
   --- | --- | --- | --- | ---
   ANY | IP addresses of interfaces through which users can authenticate. | HTTP HTTPS (Port settings must be the same as defined in the User Authentication settings for the Security Engine.) | Allow |
   ANY | IP addresses of network services that require authentication. | HTTP HTTPS | Allow | Users or User Groups who are allowed to access services, and appropriate Authentication Methods.
   ANY | IP addresses of network services that require authentication. | HTTP HTTPS | Refuse Connection tracking: Default Response: redirect to the logon page. |

5. Click Save and Install.