# Change a NetLink state manually

You can manually command NetLinks to the Enable or Disable state.

##

To change a NetLink’s state, it must be operational. You cannot send commands to NetLinks that have the unknown (gray) status.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Select Dashboard > Secure SD-WAN Dashboard.
2. Browse to Branches, and then select a branch.
3. In the ISP Information section:
   1. To enable the NetLink, select Tools > Force NetLink Enable.
   2. To disable the NetLink, select Tools > Force NetLink Disable.