# Change Access rules to allow Web Portal connections

If Web Portal connections are routed through a firewall, you must change the IPv4 Access rules in your security policy to allow them. Web Portal connections include connections to the Management Server and the Log Server as well as end-user connections.

##

For more details about the product and how to configure features, click Help or press F1.

## Steps

Allow the following connections in the IPv4 Access rules as needed:

Table 1. Access rules for the Web Portal Server
Source | Destination | Port/Service | Action
--- | --- | --- | ---
Web Portal users’ networks (or hosts) | Web Portal Server | Port defined in the Web Portal Server Properties dialog box. | Allow
Web Portal Server | Management Server | SG Control (8902-8913/TCP) | Allow
Web Portal Server | Log Server | SG Data Browsing (Web Portal Server) (8916-8917/TCP) | Allow

Note: Remember to adjust the NAT rules as well if it is necessary in your network setup.