# Element status colors

The element-level status gives an overview of the status of all engine nodes that are represented by the element (also shown for single-node components).

Table 1. Element-level status
Color | Element status | Description
--- | --- | ---
Green | All OK | All nodes have a normal status (online or standby).
Yellow | Warning | Some nodes have an abnormal status or have been commanded offline, but are still sending status updates normally.
Red | Alert | All nodes have an abnormal status, there are one or more nodes that have not sent expected status updates, or all nodes have been commanded offline.
Gray | Unknown status | No policy has been installed on any of the nodes.
White | Not monitored | An administrator has disabled monitoring for all nodes.