# Select the same Virtual Resource for multiple interfaces

You can easily use the same Virtual Resource for multiple physical or VLAN interfaces.

##

Note: This procedure is not valid for shared interfaces.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Right-click an NGFW Engine, then select Edit <element type>.
2. Browse to Interfaces.
3. Ctrl-select or shift-select multiple physical or VLAN interfaces that do not have an IP address.
4. Right-click the selected interfaces, then select Select Virtual Resource.
5. Select the Virtual Resource to associate with the interfaces, then click OK.
6. Click Save and Refresh to transfer the configuration changes.