# Add additional nodes to Master NGFW Engines

By default, the Master NGFW Engine element has two nodes on the Clustering pane of the Engine Editor. You can add new nodes to the Master NGFW Engine element. Each Master NGFW Engine supports up to 16 nodes.

## Before you begin

Install the additional physical engine device. Connect the cables for at least the interface for communication with the Management Server and the interface for communications between the clustered engines. If the device already has a working configuration from previous use, return it to the initial configuration state in the NGFW Configuration Wizard on the command line before connecting it to the network. Do not make initial contact with the Management Server before you add the node to the Master NGFW Engine configuration in the Management Client.

##

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. Select Configuration.
2. Right-click an NGFW Engine, then select Edit <element type>.
3. Browse to General > Clustering.
4. Click Add Node.
5. Give the node a unique Name.
6. In the Nodes table, double-click the IP Address, Contact IP Address, or Comment fields if you want to change the values for each NDI.
7. Click OK.
8. Click Save.
9. Save the initial configuration for the new Master NGFW Engine node to create a one-time password.
10. Make initial contact between the new Master NGFW Engine and the Management Server.
11. Refresh the policy of the Master NGFW Engine to transfer the changes to the NGFW Engines.