# SNMP traps and MIBs

You can use these SNMP traps and MIB objects with NGFW Engines.

Table 1. SNMP traps for NGFW Engines
Trap name | Objects included | Role | Description
--- | --- | --- | ---
fwPolicyInstall | fwSecurityPolicy | FW, L2FW | Policy was installed on the Firewall engine.
ipsPolicyInstall | ipsSecurityPolicy | IPS | Policy was installed on the IPS engine.
nodeBoot | - | FW, IPS, L2FW | Node bootup complete.
nodeHwmon | nodeHwmonEvent | FW, IPS, L2FW | Hardware monitoring system has detected problems.
nodeOffline | nodeOperState | FW, IPS, L2FW | Node changed to offline or standby state.
nodeOnline | nodeOperState | FW, IPS, L2FW | Node changed to online state.
nodeShutdown | - | FW, IPS, L2FW | Node is shutting down.
nodeTestFailure | nodeTestIdentity | FW, IPS, L2FW | Test subsystem reported a test failure on the node.
nodeFailedUserLogin | nodeLastLogin | FW, L2FW | Logon failed on the firewall engine's console or through SSH.
nodeUserLogin | nodeLastLogin | FW, IPS, L2FW | Log on initiated on the engine's console or through SSH.
nodeUserLogout | nodeLastLogin | FW, L2FW | Log off on the firewall engine's console or through SSH.

Table 2. Forcepoint NGFW-specific MIBs
MIB | Role | Description
--- | --- | ---
STONESOFT-SMI-MIB | - | High-level registrations MIB. This MIB defines the top-level enterprise registrations for the Forcepoint NGFW products in the .iso.org.dod.internet.private.enterprises.stonesoft branch (OID `.1.3.6.1.4.1.1369`). The other MIB modules depend on STONESOFT-SMI-MIB, so it is necessary to load STONESOFT-SMI-MIB first.
STONESOFT-NETNODE-MIB | FW, IPS, L2FW | Generic network node MIB.
STONESOFT-FIREWALL-MIB | FW, L2FW | Firewall application MIB.
STONESOFT-IPS-MIB | IPS | IPS application MIB.

NGFW Engines in the Firewall/VPN role also support objects in the following standard MIBs:

- IF-MIB (RFC 2863 and RFC 2233)
- IP-MIB (RFC 2011)
- SNMP-USER-BASED-SM-MIB (RFC 3414)
- SNMPv2 MIB (RFC 3418)