# Define FTP Protocol parameters

The FTP Protocol Agent keeps track of the ports used in File Transfer Protocol (FTP) sessions. You can also use this Protocol Agent to redirect FTP traffic to a proxy service.

##

An FTP session starts with a control connection (by default, TCP port 21), and the communications continue using a dynamically allocated port. The FTP Protocol Agent can open the actual ports used in FTP sessions as needed so that the whole range of possible dynamic ports does not need to be allowed in the policy.

For more details about the product and how to configure features, click Help or press F1.

## Steps

1. In the properties of a custom Service you have created, click Select next to the Protocol field and select FTP.
2. On the Protocol Parameters tab, set the parameters for the Protocol.
   Note: Do not change options marked as Firewall Only from their default values when you use the Service element on IPS engines or Layer 2 Firewalls.
3. Click OK.